# Propeller Object Exchange

Login | Register

### Temperature, light, proximity, position...

| Quick Links |

Contact Us
Forums
Support

Register
Login

# Sensor Object List:

| OBJECT OVERVIEW | VERSION | ATTRIBUTES | AUTHOR | PUBLISHED | UPDATED | DOWNLOADS | RATING |

1-wire Routines
1-wire device interface routines and demos. Low-level routines include network device search and CRC-8 calculation.

1.0

Cam Thompson

2006-07-18

2008-03-14

3,586

3DfixOLED
For Amateur Radio enthusiasts working with Microwaves and GPS stabilized oscillators I produced two chips for 3Dfix detection and display of other GPS parameters. The first thing I did when ...

1.04

W1AUV

2008-09-03

2008-09-04

455

6DOF Board from Sparkfun.com
This is to get the serial data from the Sparkfun.com 6DOF module. This module is very economical for a 6 degree of freedom unit.The program is self documented. Updated 5/3/09

2.0

Earl

2009-04-26

2009-05-03

115

74hc597 driver
74hc597 v1.0 Data acquisition cog reading up to 4 74hc597's in series. A 74hc597 is an 8-bit latch/shift register. It grabs digital inputs in two stages. This cog free runs ...

1.0

Cannibal Robot

2008-10-17

2008-10-17

235

A/D LTC1298
This object supports the 2 channel LTC1298 sold by Parallax. Documentation and schematic is included in the source code. Best regards, Charlie

1.0

Charles Dixon

2007-06-10

2008-07-10

1,046

AD7705 interface (ADC converter)
The AD7705 and AD7706 are complete 16-bit, low-cost, Sigma Delta ADCs intended for dc and low-frequency ac measurement applications. An integrated amplifier makes it possible to measure voltages up to ...

1.2

Jev Kuznetsov

2008-10-23

2009-06-21

282

AD8803 Octal 8-Bit Trim DAC
Interface to the AD8803 Octal 8-Bit Trim DAC.

1.0

Beau Schwabe (Parallax)

2007-08-11

2008-03-10

1,502

ADC Frequency Reader
The ADC Input Driver (http://obex.parallax.com/objects/488/) does this frequency reading and a lot more. It is also faster and is compatible with more MCP3X0X ADCs. This PASM-driven object reads values off ...

1.1

Brandon Nimon

2009-07-15

2009-08-28

75

ADC Input Driver
Driver for MCP3X0X ADCs. 1 to 8 channels, 8- to 16-bits. Functions include programmable input (Schmitt, high/low levels), frequency input, max/min values, averaging, and wait high or low input state. ...

1.31

Brandon Nimon

2009-07-22

2009-08-28

153

ADC0808driver.spin
Interfaces with National's ADC0808 analog to digital converter. Includes my debugger program and suggested connection diagram. If you're in EEE174 at CSUS you can use this code, but Dahlquist will ...

1.0

Scott Lewis

2008-12-16

2008-12-16

118

Pages: 1 2 3 4 5 6 7 8 9 10 11 12 More

Show |  | Per Page

| Copyright 2007 by Parallax, Inc. |

Please contact obex.support@parallax.com with comments or questions.