127.0.0.1	localhost
127.0.1.1	raspberrypi pi raspberry

# vehicle network
192.168.2.1	router
192.168.2.2	wsu obe obu
192.168.2.10	mabx2
192.168.2.12	pi pi1
192.168.2.15	carpc
192.168.1.77	denso pod wsu-77
192.168.2.98	winpc
192.168.2.99	linpc

# The following lines are desirable for IPv6 capable hosts
::1     ip6-localhost ip6-loopback
fe00::0 ip6-localnet
ff00::0 ip6-mcastprefix
ff02::1 ip6-allnodes
ff02::2 ip6-allrouters
